IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2016-06-21T11:14:11"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20131024_2115(x64) - Exporter 3.13.0.0 - Alternate UI 2.13.0.0"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "batyg" of Organization (no name given)
  Owner history of Person "batyg" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 1466153293 (2016-06-17T08:48:13Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCSTACKTERMINALTYPE "CGV-022" | object type "CGV-022" | names: "NBS_CordekLtd_DschrgeAndVntltngStackTrmntns_CircularGulleyVent-CGV-022:CGV-022:218774" | material: materials ("NBS_Concept_Perforated", "NBS_Concept")

Types
  IFCSTACKTERMINALTYPE "CGV-022" | 1 occurrence | material: materials ("NBS_Concept_Perforated", "NBS_Concept") | property sets: NBS_General, NBS_Data, Pset_BuildingElementProxyCommon, Pset_CoveringCommon, Pset_WallCommon

Property sets
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_DischargeAndVentilatingStackTerminations_CircularGulleyVent-CGV-022" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/vfav1jkt" (IFCTEXT)
    NBSDescription = "Discharge and ventilating stack terminations" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "90-10-60/437" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS32_ground_level_vent_box_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "90-62-24/422" (IFCTEXT)
    Uniclass2015Description = "Discharge and ventilating stack terminations" (IFCTEXT)
    Uniclass2015Reference = "Pr_65_52_61_23" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Accessories = "n/a" (IFCTEXT)
    Arrangement = "Gulley vent with perforated lid" (IFCTEXT)
    ColourOptions = "n/a" (IFCTEXT)
    ConnectionSizes = "Gas inlet: 110 mm; Water outlet: 175 mm" (IFCTEXT)
    FreeAirFlow = "7000 mm²" (IFCTEXT)
    Weight = "n/a" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 type object
    Reference = "n/a" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    Finish = "n/a" (IFCTEXT)
    Material = "Lid: Stainless steel" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
  Pset_WallCommon | properties | on 1 type object
    Reference = "n/a" (IFCTEXT)