IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2016-06-21T11:06:09"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20131024_2115(x64) - Exporter 3.13.0.0 - Alternate UI 2.13.0.0"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "batyg" of Organization (no name given)
  Owner history of Person "batyg" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 1466153293 (2016-06-17T08:48:13Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "AirBrickAndAdjustableCavityVent" | object type "AirBrickAndAdjustableCavityVent" | names: "NBS_CordekLtd_Arbrcks_AirBrickandAdjustableCavityVent:AirBrickAndAdjustableCavityVent:218868" | material: "NBS_Concept"

Types
  IFCBUILDINGELEMENTPROXYTYPE "AirBrickAndAdjustableCavityVent" | USERDEFINED | 1 occurrence | material: "NBS_Concept" | property sets: NBS_General, NBS_Data, Pset_BuildingElementProxyCommon, Pset_CoveringCommon, Pset_WallCommon

Property sets
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_Airbricks_AirBrickandAdjustableCavityVent" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/w0knsnje" (IFCTEXT)
    NBSDescription = "Airbricks" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-80-50/370" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS18_air_brick_and_cavity_vent_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-91-50/403" (IFCTEXT)
    Uniclass2015Description = "Airbricks" (IFCTEXT)
    Uniclass2015Reference = "Pr_35_90_50_03" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Accessories = "CGV-012 - Adjustable sleeve horizontal, CGV-013 - Adjustable sleeve vertical" (IFCTEXT)
    AirBrickColourOptions = "Blue/Black, Buff, Terracotta" (IFCTEXT)
    AirBrickFreeAirFlow = "7600 mm²" (IFCTEXT)
    AirBrickSize = "210 x 70 x 57 mm (l x h x d):" (IFCTEXT)
    Apertures = "Louvre" (IFCTEXT)
    Class = "n/a" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 type object
    Reference = "n/a" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    Finish = "n/a" (IFCTEXT)
    Material = "Injection moulded polypropylene" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
  Pset_WallCommon | properties | on 1 type object
    Reference = "n/a" (IFCTEXT)