IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2016-06-14T15:14:15"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1465913656 (2016-06-14T14:14:16Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1465913656 (2016-06-14T14:14:16Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_BitumenSheets_PuraflexTankVOCMembrane" | FLOOR | names: "NBS_CordekLtd_BitumenSheets_PuraflexTankVOCMembrane" | material: layers "NBS_CordekLtd_BitumenSheets_PuraflexTankVOCMembrane" ("NBS_CordekLtd_BitumenSheets_PuraflexTankVOCMembrane" 1.6) | property sets: COBie

Types
  IFCSLABTYPE "NBS_CordekLtd_BitumenSheets_PuraflexTankVOCMembrane" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_BitumenSheets_PuraflexTankVOCMembrane" ("NBS_CordekLtd_BitumenSheets_PuraflexTankVOCMembrane" 1.6) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_CoveringFlooring

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_08_08:Bitumen sheets" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "High performance hydrocarbon and chemical resistant barrier" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Provides additional waterproofing protection to the structure as part of an overall waterproofing system, robust membrane construction with excellent resistance to both puncturing and tearing" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Puraflex Tank VOC Membrane" (IFCTEXT)
    Name = "BitumenSheets_PuraflexTankVOCMembrane_CordekLtd" (IFCTEXT)
    NominalHeight = 0.44 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Polymeric composite with an adhesive bitumen layer" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 0.44 (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_Data | properties | on 1 type object
    Adhesion = "n/a" (IFCTEXT)
    BurstStrength = "145 kPa" (IFCTEXT)
    Elongation = "Longitudinal: 920%; Transverse: 780%" (IFCTEXT)
    GasRetardance = "Carbon dioxide, methane, radon and VOCs including hydrocarbons" (IFCTEXT)
    HydrostaticResistance = "758 kPa" (IFCTEXT)
    MembraneCarrierMaterial = "Polymeric composite" (IFCTEXT)
    MethaneGasPermeability = "n/a" (IFCTEXT)
    PunctureResistance = "1470 N" (IFCTEXT)
    RadonDiffusion = "n/a" (IFCTEXT)
    RollLength = "25 m" (IFCTEXT)
    Strength = "Longitudinal: 53 N/mm; Transverse: 48 N/mm" (IFCTEXT)
    TearResistance = "45 N" (IFCTEXT)
    ThirdPartyProductCertification = "n/a" (IFCTEXT)
    WaterVapourTransmission = "n/a" (IFCTEXT)
    WeightMinimum = "440 g/m²" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_BitumenSheets_PuraflexTankVOCMembrane" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/jedl4ydu" (IFCTEXT)
    NBSDescription = "Bitumen sheets" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-65-50/304" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS09_puraflex_tank_membrane_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-57-51/408" (IFCTEXT)
    Uniclass2015Description = "Bitumen sheets" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_57_08_08" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  Pset_CoveringFlooring | properties | on 1 type object
    HasAntiStaticSurface = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)