IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2016-06-14T15:15:03"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1465913703 (2016-06-14T14:15:03Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1465913703 (2016-06-14T14:15:03Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 3 elements
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-90" | FLOOR | names: "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-90" | material: layers "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-90" ("NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-90" 90.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-160" | FLOOR | names: "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-160" | material: layers "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-160" ("NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-160" 160.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-225" | FLOOR | names: "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-225" | material: layers "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-225" ("NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-225" 225.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-90" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-90" ("NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-90" 90.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_WallCommon
  IFCSLABTYPE "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-160" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-160" ("NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-160" 160.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_WallCommon
  IFCSLABTYPE "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-225" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-225" ("NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-225" 225.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_WallCommon

Property sets
  COBie | properties | on 3 objects (3 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_16:Compressible board substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Compressible EPS honeycomb with a heavy-duty polypropylene top" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Cost effective and reduced carbon footprint, less upward force is transmitted to the structure, moulded for consistent performance and durability, reduced depth and therefore less excavation, suitable for most lightweight slabs, water resistant" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cellcore HX S - 90" (IFCTEXT)
    Name = "CompressibleBoardSubstructureFormwork_CellcoreHXS-90_CordekLtd" (IFCTEXT)
    NominalHeight = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x 1200 x 90 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_16:Compressible board substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Compressible EPS honeycomb with a heavy-duty polypropylene top" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Cost effective and reduced carbon footprint, less upward force is transmitted to the structure, moulded for consistent performance and durability, reduced depth and therefore less excavation, suitable for most lightweight slabs, water resistant" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cellcore HX S - 160" (IFCTEXT)
    Name = "CompressibleBoardSubstructureFormwork_CellcoreHXS-160_CordekLtd" (IFCTEXT)
    NominalHeight = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x 1200 x 160 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_16:Compressible board substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Compressible EPS honeycomb with a heavy-duty polypropylene top" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Cost effective and reduced carbon footprint, less upward force is transmitted to the structure, moulded for consistent performance and durability, reduced depth and therefore less excavation, suitable for most lightweight slabs, water resistant" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cellcore HX S - 225" (IFCTEXT)
    Name = "CompressibleBoardSubstructureFormwork_CellcoreHXS-225_CordekLtd" (IFCTEXT)
    NominalHeight = 225. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x 1200 x 225 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene (EPS) honeycomb with a heavy-duty polypropylene top" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 90. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene (EPS) honeycomb with a heavy-duty polypropylene top" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 160. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene (EPS) honeycomb with a heavy-duty polypropylene top" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 225. (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_Data | properties | on 3 type objects
    Applications = "For use beneath reinforced concrete floor slabs" (IFCTEXT)
    GradeOptions = "7/10 (safe load/fail load), 9/13 (safe load/fail load), 13/18 (safe load/fail load), 18/24 (safe load/fail load), 24/32 (safe load/fail load)" (IFCTEXT)
    InsulationThermalResistance = "n/a" (IFCTEXT)
    InsulationThickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RecycledContentMinimum = "n/a" (IFCTEXT)
    ThirdPartyCertification = "BBA Certificate - 11/4862" (IFCTEXT)
    WidthOptions = "n/a" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-90" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/nvytkbgb" (IFCTEXT)
    NBSDescription = "Compressible board substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/390" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS03_cellcore_hx_data_sheet_cordek_v3.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/416" (IFCTEXT)
    Uniclass2015Description = "Compressible board substructure formwork" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_16" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-160" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/nvytkbgb" (IFCTEXT)
    NBSDescription = "Compressible board substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/390" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS03_cellcore_hx_data_sheet_cordek_v3.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/416" (IFCTEXT)
    Uniclass2015Description = "Compressible board substructure formwork" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_16" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_CompressibleBoardSubstructureFormwork_CellcoreHXS-225" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/nvytkbgb" (IFCTEXT)
    NBSDescription = "Compressible board substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/390" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS03_cellcore_hx_data_sheet_cordek_v3.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/416" (IFCTEXT)
    Uniclass2015Description = "Compressible board substructure formwork" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_16" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  Pset_WallCommon | properties | on 3 type objects
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCREAL)