IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2016-06-14T15:15:06"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1465913706 (2016-06-14T14:15:06Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1465913706 (2016-06-14T14:15:06Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_EPSBoard_FilcorEPS" | FLOOR | names: "NBS_CordekLtd_EPSBoard_FilcorEPS" | material: layers "NBS_CordekLtd_EPSBoard_FilcorEPS" ("NBS_CordekLtd_EPSBoard_FilcorEPS" 25.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_CordekLtd_EPSBoard_FilcorEPS" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_EPSBoard_FilcorEPS" ("NBS_CordekLtd_EPSBoard_FilcorEPS" 25.) | property sets: COBie, Pset_CoveringCommon, NBS_General, NBS_Data

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_63_26:Expanded polystyrene (EPS) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Expanded polystyrene insulation" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Lightweight and easy to handle, available as standard sheets or blocks, can be profiled to customer requirements, provides a high degree of insulation, fire retardant version available" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Filcor EPS" (IFCTEXT)
    Name = "EPSBoard_FilcorEPS_CordekLtd" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x 1200 mm x Required Depth" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene (EPS)" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 25. (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_EPSBoard_FilcorEPS" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/nsehilwg" (IFCTEXT)
    NBSDescription = "Expanded polystyrene (EPS) board" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-45-65/380" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS31_filcor_data_sheet_v1_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-63/429" (IFCTEXT)
    Uniclass2015Description = "Expanded polystyrene (EPS) boards" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_63_26" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    CompressiveStrengthAt10Deformation = "Filcor 20: 20 kPa; Filcor 45: 45 kPa; Filcor 70: 70 kPa; Filcor 90: 90 kPa; Filcor 100: 100 kPa; Filcor 120: 120 kPa; Filcor 140: 140 kPa; Filcor 160: 160 kPa; Filcor 190: 190 kPa" (IFCTEXT)
    Density = "Filcor 20: 15 kg/m³; Filcor 45: 20 kg/m³; Filcor 70: 25 kg/m³; Filcor 90: 30 kg/m³; Filcor 100: 35 kg/m³; Filcor 120: 40 kg/m³; Filcor 140: 45 kg/m³; Filcor 160: 50 kg/m³; Filcor 190: 55 kg/m³" (IFCTEXT)
    Facing = "n/a" (IFCTEXT)
    GradeOptions = "Filcor 20, Filcor 45, Filcor 70, Filcor 90, Filcor 100, Filcor 120, Filcor 140, Filcor 160, Filcor 190" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    ThermalConductivityMaximum = "Filcor 20: 0.038 W/mK; Filcor 45: 0.036 W/mK; Filcor 70: 0.035 W/mK; Filcor 90: 0.034 W/mK; Filcor 100 and Filcor 120: 0.033 W/mK; Filcor 140, Filcor 160 and Filcor 190: 0.032 W/mK" (IFCTEXT)
    ThicknessOptions = "Available 25-1200 mm" (IFCTEXT)
    ThirdPartyCertification = "n/a" (IFCTEXT)