IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2016-06-14T15:14:15"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1465913656 (2016-06-14T14:14:16Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1465913656 (2016-06-14T14:14:16Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_GasResistantDampProofCoursesAndOrCavityTrays_GasResistantDPC" | FLOOR | names: "NBS_CordekLtd_GasResistantDampProofCoursesAndOrCavityTrays_GasResistantDPC" | material: layers "NBS_CordekLtd_GasResistantDampProofCoursesAndOrCavityTrays_GasResistantDPC" ("NBS_CordekLtd_GasResistantDampProofCoursesAndOrCavityTrays_GasResistantDPC" 1.6) | property sets: COBie

Types
  IFCSLABTYPE "NBS_CordekLtd_GasResistantDampProofCoursesAndOrCavityTrays_GasResistantDPC" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_GasResistantDampProofCoursesAndOrCavityTrays_GasResistantDPC" ("NBS_CordekLtd_GasResistantDampProofCoursesAndOrCavityTrays_GasResistantDPC" 1.6) | property sets: COBie, Pset_CoveringCommon, NBS_General, NBS_Data, Pset_WallCommon

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_21_35:Gas-resistant damp-proof courses" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Polymeric gas resistant DPC" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Excellent all round physical properties, flexible even at low temperatures, good mortar adhesion properties" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Gas Resistant DPC" (IFCTEXT)
    Name = "GasResistantDampProofCoursesAndOrCavityTrays_GasResistantDPC_CordekLtd" (IFCTEXT)
    NominalHeight = 0.6 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Polymeric" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 0.6 (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_GasResistantDampProofCoursesAndOrCavityTrays_GasResistantDPC" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/lyj5jfky" (IFCTEXT)
    NBSDescription = "Gas-resistant damp proof courses and/ or cavity trays" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-25-20/330" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS13_gas_resistant_dpc_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-57-21/445" (IFCTEXT)
    Uniclass2015Description = "Gas-resistant damp-proof courses" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_57_21_35" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    BurstStrength = "n/a" (IFCTEXT)
    Compatibility = "Suitable for use with MB420, Gas Resistant Self Adhesive and Radon Membranes" (IFCTEXT)
    Elongation = "6" (IFCTEXT)
    HydrostaticResistance = "n/a" (IFCTEXT)
    ImpactResistance = "250 mm" (IFCTEXT)
    JointStrength = "153 N/50 mm" (IFCTEXT)
    LowTemperatureResistance = "-40°C" (IFCTEXT)
    MethaneGasPermeability = "1.16 x 10^-14" (IFCTEXT)
    PerformanceCriteria = "Carbon dioxide, methane and radon" (IFCTEXT)
    PunctureResistance = "n/a" (IFCTEXT)
    RollLength = "20 m" (IFCTEXT)
    RollWidthOptions = "Available 100–1000 mm" (IFCTEXT)
    StaticLoadResistance = "20 kg" (IFCTEXT)
    TearResistance = "270 N" (IFCTEXT)
    TensileStrength = "15 N/mm²" (IFCTEXT)
    ThirdPartyCertification = "n/a" (IFCTEXT)
    WaterVapourTransmission = "0.5 g/m²/day" (IFCTEXT)
    WeightMinimum = "n/a" (IFCTEXT)
  Pset_WallCommon | properties | on 1 type object
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCREAL)