IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2016-06-14T15:15:04"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1465913705 (2016-06-14T14:15:05Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1465913705 (2016-06-14T14:15:05Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 3 elements
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-135" | FLOOR | names: "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-135" | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-135" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-135" 135.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-205" | FLOOR | names: "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-205" | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-205" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-205" 205.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-270" | FLOOR | names: "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-270" | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-270" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-270" 270.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-135" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-135" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-135" 135.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_CoveringFlooring
  IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-205" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-205" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-205" 205.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_CoveringFlooring
  IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-270" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-270" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-270" 270.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_CoveringFlooring

Property sets
  COBie | properties | on 3 objects (3 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_37:High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Expanded polystyrene: White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Gas venting and ground heave protection board" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Light, robust and easy to install panels, all variations include drainage slots to alleviate water pressure, unaffected by both UV light and water, can be connected to the Cordek range of perimeter vents" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cellvent HX - 135" (IFCTEXT)
    Name = "HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-135_CordekLtd" (IFCTEXT)
    NominalHeight = 135. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x 1200 x 135 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_37:High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Expanded polystyrene: White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Gas venting and ground heave protection board" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Light, robust and easy to install panels, all variations include drainage slots to alleviate water pressure, unaffected by both UV light and water, can be connected to the Cordek range of perimeter vents" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cellvent HX - 205" (IFCTEXT)
    Name = "HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-205_CordekLtd" (IFCTEXT)
    NominalHeight = 205. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x 1200 x 205 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_37:High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Expanded polystyrene: White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Gas venting and ground heave protection board" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Light, robust and easy to install panels, all variations include drainage slots to alleviate water pressure, unaffected by both UV light and water, can be connected to the Cordek range of perimeter vents" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cellvent HX - 270" (IFCTEXT)
    Name = "HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-270_CordekLtd" (IFCTEXT)
    NominalHeight = 270. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "2400 x 1200 x 270 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene (EPS) and heavy-duty polypropylene" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 135. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene (EPS) and heavy-duty polypropylene" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 205. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene (EPS) and heavy-duty polypropylene" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 270. (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_Data | properties | on 3 type objects
    Applications = "For use below suitably reinforced ground floor slabs" (IFCTEXT)
    GradeOptions = "7/10 (safe load/fail load), 9/13 (safe load/fail load), 13/18 (safe load/fail load), 18/24 (safe load/fail load)" (IFCTEXT)
    LoadbearingCapacityInfo = "Dependent on grade" (IFCTEXT)
    RecycledContentMinimum = "n/a" (IFCTEXT)
    ThermalResistance = "n/a" (IFCTEXT)
    ThirdPartyProductCertification = "n/a" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-135" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/n2fazk0m" (IFCTEXT)
    NBSDescription = "High density expanded polystyrene ventilated substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/400" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS05_cellvent_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/437" (IFCTEXT)
    Uniclass2015Description = "High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_37" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-205" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/n2fazk0m" (IFCTEXT)
    NBSDescription = "High density expanded polystyrene ventilated substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/400" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS05_cellvent_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/437" (IFCTEXT)
    Uniclass2015Description = "High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_37" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_CellventHX-270" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/n2fazk0m" (IFCTEXT)
    NBSDescription = "High density expanded polystyrene ventilated substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/400" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS05_cellvent_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/437" (IFCTEXT)
    Uniclass2015Description = "High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_37" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  Pset_CoveringFlooring | properties | on 3 type objects
    HasAntiStaticSurface = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)