IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2016-06-14T15:15:04"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1465913705 (2016-06-14T14:15:05Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1465913705 (2016-06-14T14:15:05Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 4 elements
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-80" | FLOOR | names: "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-80" | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-80" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-80" 80.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-100" | FLOOR | names: "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-100" | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-100" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-100" 100.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-150" | FLOOR | names: "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-150" | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-150" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-150" 150.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-200" | FLOOR | names: "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-200" | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-200" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-200" 200.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-80" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-80" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-80" 80.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_CoveringFlooring
  IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-100" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-100" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-100" 100.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_CoveringFlooring
  IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-150" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-150" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-150" 150.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_CoveringFlooring
  IFCSLABTYPE "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-200" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-200" ("NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-200" 200.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_CoveringFlooring

Property sets
  COBie | properties | on 4 objects (4 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_37:High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Passive gas venting substrate for use under ground bearing and suspended ground floor slabs" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Light, robust and easy to install panels, unaffected by both UV light and water and are flame retardant" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Ventform - 80" (IFCTEXT)
    Name = "HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-80_CordekLtd" (IFCTEXT)
    NominalHeight = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Square" (IFCTEXT)
    Size = "1200 x 1200 x 80 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_37:High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Passive gas venting substrate for ground bearing and suspended ground floor slabs" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Light, robust and easy to install panels, unaffected by both UV light and water and are flame retardant" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Ventform - 100" (IFCTEXT)
    Name = "HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-100_CordekLtd" (IFCTEXT)
    NominalHeight = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Square" (IFCTEXT)
    Size = "1200 x 1200 x 100 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_37:High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Passive gas venting substrate for use under suspended ground floor slabs" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Light, robust and easy to install panels, unaffected by both UV light and water and are flame retardant" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Ventform - 150" (IFCTEXT)
    Name = "HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-150_CordekLtd" (IFCTEXT)
    NominalHeight = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Square" (IFCTEXT)
    Size = "1200 x 1200 x 150 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_37:High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Passive gas venting substrate for use under suspended ground floor slabs" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Light, robust and easy to install panels, unaffected by both UV light and water and are flame retardant" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Ventform - 200" (IFCTEXT)
    Name = "HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-200_CordekLtd" (IFCTEXT)
    NominalHeight = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Square" (IFCTEXT)
    Size = "1200 x 1200 x 200 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene (EPS)" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 80. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene (EPS)" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene (EPS)" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 150. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Expanded polystyrene (EPS)" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 200. (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_Data | properties | on 1 type object
    Applications = "For use under suitably reinforced concrete ground floor slabs" (IFCTEXT)
    GradeOptions = "80/20 (depth/maximum load), 80/30 (depth/maximum load), 80/40 (depth/maximum load), 80/50 (depth/maximum load)" (IFCTEXT)
    LoadbearingCapacityInfo = "80/20: 20 kN/m²; 80/30: 30 kN/m²; 80/40: 40 kN/m²; 80/50: 50 kN/m²" (IFCTEXT)
    RecycledContentMinimum = "n/a" (IFCTEXT)
    ThermalResistance = "80/20: 1.60 m²K/W; 80/30: 1.65 m²K/W; 80/40: 1.69 m²K/W; 80/50: 1.75 m²K/W" (IFCTEXT)
    ThirdPartyProductCertification = "BBA Certificate - 12/4916" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "For use under suitably reinforced concrete ground floor slabs" (IFCTEXT)
    GradeOptions = "100/20 (depth/maximum load),100/30 (depth/maximum load), 100/40 (depth/maximum load), 100/50 (depth/maximum load)" (IFCTEXT)
    LoadbearingCapacityInfo = "100/20: 20 kN/m²; 100/30: 30 kN/m²; 100/40: 40 kN/m²; 100/50: 50 kN/m²" (IFCTEXT)
    RecycledContentMinimum = "n/a" (IFCTEXT)
    ThermalResistance = "100/20: 1.84 m²K/W; 100/30: 1.90 m²K/W; 100/40: 1.95 m²K/W; 100/50: 2.01 m²K/W" (IFCTEXT)
    ThirdPartyProductCertification = "BBA Certificate - 12/4916" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "For use under suspended ground floor slabs" (IFCTEXT)
    GradeOptions = "150/9 (depth/maximum load),150/13 (depth/maximum load)" (IFCTEXT)
    LoadbearingCapacityInfo = "150/9: 9 kN/m²; 150/13: 13 kN/m²" (IFCTEXT)
    RecycledContentMinimum = "n/a" (IFCTEXT)
    ThermalResistance = "150/9: 2.37 m²K/W; 150/13: 2.43 m²K/W" (IFCTEXT)
    ThirdPartyProductCertification = "BBA Certificate - 12/4916" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "For use under suspended ground floor slabs" (IFCTEXT)
    GradeOptions = "200/9 (depth/maximum load), 200/13 (depth/maximum load)" (IFCTEXT)
    LoadbearingCapacityInfo = "200/9: 9 kN/m²; 200/13: 13 kN/m²" (IFCTEXT)
    RecycledContentMinimum = "n/a" (IFCTEXT)
    ThermalResistance = "200/9: 2.63 m²K/W; 200/13: 2.70 m²K/W" (IFCTEXT)
    ThirdPartyProductCertification = "BBA Certificate - 12/4916" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-80" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/co43t14w" (IFCTEXT)
    NBSDescription = "High density expanded polystyrene ventilated substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/400" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS06_ventform_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/437" (IFCTEXT)
    Uniclass2015Description = "High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_37" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-100" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/co43t14w" (IFCTEXT)
    NBSDescription = "High density expanded polystyrene ventilated substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/400" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS06_ventform_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/437" (IFCTEXT)
    Uniclass2015Description = "High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_37" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-150" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/co43t14w" (IFCTEXT)
    NBSDescription = "High density expanded polystyrene ventilated substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/400" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS06_ventform_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/437" (IFCTEXT)
    Uniclass2015Description = "High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_37" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_HighDensityExpandedPolystyreneVentilatedSubstructureFormwork_Ventform-200" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/co43t14w" (IFCTEXT)
    NBSDescription = "High density expanded polystyrene ventilated substructure formwork" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/400" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS06_ventform_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/437" (IFCTEXT)
    Uniclass2015Description = "High density expanded polystyrene (HDPS) ventilated substructure formwork" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_37" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  Pset_CoveringFlooring | properties | on 4 type objects
    HasAntiStaticSurface = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)