IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2016-06-14T15:15:05"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1465913705 (2016-06-14T14:15:05Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1465913705 (2016-06-14T14:15:05Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 3 elements
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_PIF_CellformHX-85" | FLOOR | names: "NBS_CordekLtd_PIF_CellformHX-85" | material: layers "NBS_CordekLtd_PIF_CellformHX-85" ("NBS_CordekLtd_PIF_CellformHX-85" 85.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_PIF_CellformHX-155" | FLOOR | names: "NBS_CordekLtd_PIF_CellformHX-155" | material: layers "NBS_CordekLtd_PIF_CellformHX-155" ("NBS_CordekLtd_PIF_CellformHX-155" 155.) | property sets: COBie
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_PIF_CellformHX-220" | FLOOR | names: "NBS_CordekLtd_PIF_CellformHX-220" | material: layers "NBS_CordekLtd_PIF_CellformHX-220" ("NBS_CordekLtd_PIF_CellformHX-220" 220.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_CordekLtd_PIF_CellformHX-85" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_PIF_CellformHX-85" ("NBS_CordekLtd_PIF_CellformHX-85" 85.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_WallCommon
  IFCSLABTYPE "NBS_CordekLtd_PIF_CellformHX-155" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_PIF_CellformHX-155" ("NBS_CordekLtd_PIF_CellformHX-155" 155.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_WallCommon
  IFCSLABTYPE "NBS_CordekLtd_PIF_CellformHX-220" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_PIF_CellformHX-220" ("NBS_CordekLtd_PIF_CellformHX-220" 220.) | property sets: COBie, Pset_CoveringCommon, NBS_Data, NBS_General, Pset_WallCommon

Property sets
  COBie | properties | on 3 objects (3 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_62:Permanent insulation formwork (PIF)" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Cellcore HX B: White" (IFCTEXT)
    Constituents = "Cellcore HX B, Groundform" (IFCTEXT)
    Description = "Combined heave protection and permanent formwork" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Manufactured to suit ground beam dimensions, range of accessories available" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cellform HX - 85" (IFCTEXT)
    Name = "PIF_CellformHX-85_CordekLtd" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_62:Permanent insulation formwork (PIF)" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Cellcore HX B: White" (IFCTEXT)
    Constituents = "Cellcore HX B, Groundform" (IFCTEXT)
    Description = "Combined heave protection and permanent formwork" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Manufactured to suit ground beam dimensions, range of accessories available" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cellform HX - 155" (IFCTEXT)
    Name = "PIF_CellformHX-155_CordekLtd" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_29_62:Permanent insulation formwork (PIF)" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Cellcore HX B: White" (IFCTEXT)
    Constituents = "Cellcore HX B, Groundform" (IFCTEXT)
    Description = "Combined heave protection and permanent formwork" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Manufactured to suit ground beam dimensions, range of accessories available" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cellform HX - 220" (IFCTEXT)
    Name = "PIF_CellformHX-220_CordekLtd" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Cellcore HX B: Compressible EPS honeycomb with a heavy-duty polypropylene top" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 85. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Cellcore HX B: Compressible EPS honeycomb with a heavy-duty polypropylene top" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 155. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Cellcore HX B: Compressible EPS honeycomb with a heavy-duty polypropylene top" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 220. (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_Data | properties | on 2 type objects
    Applications = "For use as a combined ground heave protection and permanent formwork system for the construction of ground beams" (IFCTEXT)
    BoardGradeOptions = "7/10 (safe load/fail load), 9/13 (safe load/fail load), 13/18 (safe load/fail load), 18/24 (safe load/fail load), 24/32 (safe load/fail load)" (IFCTEXT)
    BoardThickness = "155 mm" (IFCTEXT)
    DensityMinimum = "n/a" (IFCTEXT)
    DesignationFireRetardantClass = "n/a" (IFCTEXT)
    DesignationStructure = "n/a" (IFCTEXT)
    SizeOptions = "Manufactured to suit beam requirements" (IFCTEXT)
    ThirdPartyProductCertification = "BBA Certificate - 11/4862" (IFCTEXT)
    WallWidthOverall = "Dependent on beam requirements" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "For use as a combined ground heave protection and permanent formwork system for the construction of ground beams" (IFCTEXT)
    BoardGradeOptions = "7/10 (safe load/fail load), 9/13 (safe load/fail load), 13/18 (safe load/fail load), 18/24 (safe load/fail load), 24/32 (safe load/fail load)" (IFCTEXT)
    BoardThickness = "85 mm" (IFCTEXT)
    DensityMinimum = "n/a" (IFCTEXT)
    DesignationFireRetardantClass = "n/a" (IFCTEXT)
    DesignationStructure = "n/a" (IFCTEXT)
    SizeOptions = "Manufactured to suit beam requirements" (IFCTEXT)
    ThirdPartyProductCertification = "BBA Certificate - 11/4862" (IFCTEXT)
    WallWidthOverall = "Dependent on beam requirements" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_PIF_CellformHX-85" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/vaefhqq5" (IFCTEXT)
    NBSDescription = "Permanent insulation formwork (PIF)" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/420" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/products/cellform-hx" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/462" (IFCTEXT)
    Uniclass2015Description = "Permanent insulation formwork (PIF)" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_62" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_PIF_CellformHX-155" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/vaefhqq5" (IFCTEXT)
    NBSDescription = "Permanent insulation formwork (PIF)" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/420" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/products/cellform-hx" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/462" (IFCTEXT)
    Uniclass2015Description = "Permanent insulation formwork (PIF)" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_62" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_PIF_CellformHX-220" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/vaefhqq5" (IFCTEXT)
    NBSDescription = "Permanent insulation formwork (PIF)" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-50-30/420" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/products/cellform-hx" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-71-29/462" (IFCTEXT)
    Uniclass2015Description = "Permanent insulation formwork (PIF)" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_71_29_62" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  Pset_WallCommon | properties | on 3 type objects
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCREAL)