IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2019-07-02T15:11:29"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1562076690 (2019-07-02T14:11:30Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1562076690 (2019-07-02T14:11:30Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_PlasticsSheets_TriGasMembrane" | FLOOR | names: "NBS_CordekLtd_PlasticsSheets_TriGasMembrane" | material: layers "NBS_CordekLtd_PlasticsSheets_TriGasMembrane" ("NBS_CordekLtd_PlasticsSheets_TriGasMembrane" 1.6) | property sets: COBie

Types
  IFCSLABTYPE "NBS_CordekLtd_PlasticsSheets_TriGasMembrane" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_PlasticsSheets_TriGasMembrane" ("NBS_CordekLtd_PlasticsSheets_TriGasMembrane" 1.6) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_65_60:Plastics sheets" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Green, Silver" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Tri-Gas Membrane is a high performance gas membrane for use in situations where resistance to methane, carbon dioxide and/or radon gas is required" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    Material = "Reinforced low density polyethylene with an aluminium foil core" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Tri-Gas Membrane" (IFCTEXT)
    Name = "PlasticsSheets_Tri-GasMembrane_CordekLtd" (IFCTEXT)
    NominalHeight = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 50000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "2000 x 50000 x 0.4 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = TRUE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_Cordek Ltd_PlasticsSheets_TriGasMembrane" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/j1te2kqh" (IFCTEXT)
    NBSDescription = "Plastics sheets" (IFCTEXT)
    NBSReference = "45-65-50/325" (IFCTEXT)
    ProductInformation = "https://cordek.com/products/tri-gas-membrane1" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_57_65_60" (IFCTEXT)
    Uniclass2015Title = "Plastics sheets" (IFCTEXT)
    Uniclass2015Version = "Products v1.14" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    COGasPermeability = "0.195" (IFCTEXT)
    Form = "n/a" (IFCTEXT)
    MethaneGasPermeability = "0.041" (IFCTEXT)
    PerformanceAntistaticProperties = "n/a" (IFCTEXT)
    PerformanceElongationToBreak = "22% (MD), 16% (XD)" (IFCTEXT)
    PerformanceResistantToUndergroundGases = "n/a" (IFCTEXT)
    PerformanceTearResistance = "295 N (MD), 341 N (XD)" (IFCTEXT)
    PerformanceTensileStrength = "370 N/mm (MD), 347 N/mm (XD)" (IFCTEXT)
    PerformanceUvStabilization = "n/a" (IFCTEXT)
    PerformanceWaterVapourResistance = "0.01 gsm/day" (IFCTEXT)
    PhysicalPropertiesDimensionsRollLength = "50000 mm" (IFCTEXT)
    PhysicalPropertiesDimensionsThickness = "0.4 mm" (IFCTEXT)
    PhysicalPropertiesDimensionsWidth = "2000 mm" (IFCTEXT)
    PhysicalPropertiesWeight = "370 gsm" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    RollWeight = "38 kg" (IFCTEXT)
    RootInhibitor = "n/a" (IFCTEXT)
    Standard = "n/a" (IFCTEXT)
    TemperatureRange = "-40 to +70" (IFCTEXT)
    ThirdPartyCertification = "n/a" (IFCTEXT)