IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2016-06-14T15:14:16"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1465913657 (2016-06-14T14:14:17Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1465913657 (2016-06-14T14:14:17Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CordekLtd_PolyethyleneCompositeGasRetardantSheets_RadonMembrane" | FLOOR | names: "NBS_CordekLtd_PolyethyleneCompositeGasRetardantSheets_RadonMembrane" | material: layers "NBS_CordekLtd_PolyethyleneCompositeGasRetardantSheets_RadonMembrane" ("NBS_CordekLtd_PolyethyleneCompositeGasRetardantSheets_RadonMembrane" 1.6) | property sets: COBie

Types
  IFCSLABTYPE "NBS_CordekLtd_PolyethyleneCompositeGasRetardantSheets_RadonMembrane" | FLOOR | 1 occurrence | material: layers "NBS_CordekLtd_PolyethyleneCompositeGasRetardantSheets_RadonMembrane" ("NBS_CordekLtd_PolyethyleneCompositeGasRetardantSheets_RadonMembrane" 1.6) | property sets: COBie, Pset_CoveringCommon, NBS_General, NBS_Data, Pset_CoveringFlooring

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_61_65:Polyethylene composite gas retardant sheets" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Blue" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "High performance gas membrane" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Provides additional damp proofing protection to the structure, robust membrane with a high resistance to damage and puncturing" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cordek.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Radon Membrane" (IFCTEXT)
    Name = "PolyethyleneCompositeGasRetardantSheets_RadonMembrane_CordekLtd" (IFCTEXT)
    NominalHeight = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 25000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CordekLtd_PolyethyleneCompositeGasRetardantSheets_RadonMembrane" (IFCTEXT)
    ManufacturerName = "Cordek Ltd" (IFCTEXT)
    ManufacturerURL = "www.cordek.com" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/0tvbcvgp" (IFCTEXT)
    NBSDescription = "Polyethylene composite gas retardant sheets" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-65-50/359" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cordek.com/uploads/data_sheets/M-DS14_radon_membrane_data_sheet_v2_cordek.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-57-51/463" (IFCTEXT)
    Uniclass2015Description = "Polyethylene composite gas retardant sheets" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_57_61_65" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    BurstStrength = "n/a" (IFCTEXT)
    Elongation = "Longitudinal: 230%; Transverse:235%" (IFCTEXT)
    HydrostaticResistance = "n/a" (IFCTEXT)
    MethaneGasPermeability = "n/a" (IFCTEXT)
    PerformanceCriteria = "Radon" (IFCTEXT)
    PhysicalPropertiesTearResistance = "n/a" (IFCTEXT)
    PhysicalPropertiesTensileStrength = ">9.9 N/50 mm" (IFCTEXT)
    PhysicalPropertiesWeight = "n/a" (IFCTEXT)
    PunctureResistance = "n/a" (IFCTEXT)
    ThirdPartyCertification = "n/a" (IFCTEXT)
  Pset_CoveringFlooring | properties | on 1 type object
    HasAntiStaticSurface = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)